**ARTIC WOLF / FOX SOFT COOLER**

**Instructions for Use**

1. Wire the electrical connection into the vehicles wiring system via an on/off toggle switch (user supplied).

 Brown to Positive Blue to Ground

We recommend using a 5-amp fuse on the positive side for overcurrent protection.

1. Verify inside of bladder is clean and free of debris and add items below.

 Fox 2L 16 ounces of water

 1.5 pounds of ice

 2 ounces of Paragon Pro Defense solution

 Fox 6L 32 ounces of water

 3 pounds of ice

 2 ounces of Paragon Pro Defense solution

 Wolf 6L 32 ounces of water

 5 pounds of ice

 2 ounces of Paragon Pro Defense solution

 Wolf 10L 64 ounces of water

 9-10 pounds of ice

 2 ounces of Paragon Pro Defense solution

1. Connect the male connectors from the garment into the female connectors on the bag. A water supply hose may be added for remote mounted bags. An audible click can be heard when the connectors are properly connected.
2. Power the system on.

**Preventive Care and Maintenance**

1. Empty water and clean inside of bladder. Let bladder air dry.
2. For periods of longer storage, pour water into bladder and add 16oz. of Paragon Pro Defense solution.
3. Cycle water & solution mix throughout system for ten minutes.
4. Empty bladder and allow to completely air dry before putting into storage.

**Popular Accessories**

* 01-50000 Defense 16 ounce bottle
* 01-51000 Everlast Ice
* 53-40000 Drain kit
* 31-41000 Guardian Bulkhead connector

1146 Carding Machine Road Loudon, Tennessee 37774

865.643.8700

[www.paragonproinc.com](http://www.paragonproinc.com/)